AR checking written on:
'C:\Users\JD\Documents\stewy\stewy's head\stewy's head_AR-Check.txt'
'action_menu_annular_check.py'
version = 1.7.2
Testing PCB for Annular Rings
TH Pads >= 0.125 Vias >= 0.125
PHD margin on PTH = 0

VIAS that Pass = 0; Fails = 0
TH PADS that Pass = 21; Fails = 0
NPTH PADS that Pass = 0; Fails = 0
